Raspberry Pi Documentation

Both Pi’s:

* Raspberry Pi OS 32-bit, scadabr w/ desktop, and openplc is running lite
* SSH enabled w/ password authentication
* Auto Login at boot
* NetworkManager is set to manage networking, and sets the static IP addresses

Pi 1:

* Hostname & Username: scadabr
* Pw: scadabr
* IP: Static 192.168.8.1/24 on eth0
* Wifi IP: 10.4.152.2
* 32gb SD card
* Software installed:
  + ScadaBR .zip Linux installer from <https://github.com/ScadaBR/ScadaBR/releases/tag/v1.2>
* Eth0 MAC: b8:27:eb:17:03:e1
* wlan0 MAC: b8:27:eb:42:56:b4

Pi 2:

* Hostname & Username: openplc
* Pw: openplc
* IP: Static 192.168.8.2/24 on eth0
* Wifi IP: 10.4.176.212
* 8gb SD card
* Software installed:
  + OpenPLC Runtime <https://github.com/thiagoralves/OpenPLC_v3>
  + WiringPi, required for OpenPLC Runtime <https://github.com/WiringPi/WiringPi>
* eth0 MAC: b8:27:eb:7d:5c:24
* wlan0 MAC: b8:27:eb:28:09:71